Durban

Manufacturing process

**1/10” loop pile**

Pile content

**60 % PA/ 40 % PP**

Primary backing

**Twinback**

Pile weight

**± 660 gr./m²**

Total weight

**± 1.800 gr./m²**

Pile height

**± 3 mm**

Total height

**± 7 mm**

Tuft density/m²

**± 225 000**

Width

**400 + 500 cm**

Sound insulation

**± 22 dB**

Fire class

**Cfl-s1 (EN 13501-1)**

only with full adhesion



