Castor

Manufacturing process

**Tufted synthetic grass**

Pile content

**100 % PP**

Secondary backing

**Nops**

Pile weight

**ca. 1.100 gr./m²**

Total weight

**ca. 1.985 gr./m²**

Pile height

**ca. 30 mm**

Width

**300 cm**

****