Nevada



Manufacturing process

**1/10” Tufted loop pile**

Pile content

**100 % Polyamid**

Primary backing

**Bitumen**

Pile weight

**ca. 550 gr./m²**

Total weight

**ca. 4.000 gr./m²**

Pile height

**ca. 3 mm**

Total height

**ca. 5 mm**

Tuft density/m²

**ca. 177 750**

Size

**50 x 50 cm**



