Texas

****

Manufacturing process

**1/10” Tufted loop pile**

Pile content

**100 % PP**

Primary backing

**Bitumen**

Pile weight

**ca. 400 gr./m²**

Total weight

**ca. 3.700 gr./m²**

Pile height

**ca. 2,9 mm**

Total height

**ca. 5,9 mm**

Size

**50 x 50 cm**

Fire class

**Cfl-s1**

