Timeless

****

Manufacturing process

**Tufting 1/8” cutpile**

Pile content

**100 % PP**

Primary backing

**Woven PP**

Secondary backing

**Synthetic backing**

Pile weight

**Ca 2.100 gr./m²**

Total weight

**Ca 2.945 gr./m²**

Pile height

**Ca 12 mm**

Total height

**Ca 15 mm**

Tuft density

**Ca 133 875/m²**

Width

**400 cm**

Sound insulation

**28 dB**

Fire class

**EN 13501-1**





